For 1990-2009 cars

1. Disassemble the input and third sprag clutch assemblies (653, 665) from the input clutch housing assembly (632).

Important: After you remove the spiral lock retaining ring (717), discard the ring. Use a new spiral lock retaining ring when you reassemble the sprag.

2. Use a tapered blade screwdriver in order to remove the spiral lock retaining ring (717) from the input clutch sprag outer race retainer.
3. Remove the third clutch sprag assembly (665) and the input clutch sprag assembly (653) from the input and third clutch sprag inner race (661).
4. Remove the input and third clutch sprag inner race (661) and the input sun gear spacer (667) from the input sun gear (668).
5. Remove the 3rd clutch sprag outer race retainer (718).
6. Remove the input and third clutch sprag end bearings (719) and the input and third clutch sprag center bearing (721) from the sprag outer races (653, 665).

Important: Do not disassemble the sprag elements.

7. Remove the 3rd clutch and input clutch sprag assemblies (720, 722) from the sprag outer races (653, 665).