For 1990-2009 cars

### Removal Procedure

1. Remove the left closeout/insulator pane. Refer to Instrument Panel Insulator Panel Replacement - Left Side
2. Remove the accelerator controls cable (5) from accelerator controls pedal (1).
3. Remove the bolt (3) and stud (2) holding the accelerator controls pedal to the bulkhead (4).
4. Remove the accelerator controls pedal (1) from the bulkhead (4).

### Installation Procedure

1. Install the accelerator controls pedal (1) to the bulkhead (4).

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

2. Install the bolt (3) and stud (2) holding the accelerator controls pedal to the bulkhead (4).

Tighten
Tighten the stud and bolt to 3 (27 lb in).

3. Install the accelerator controls cable (5) to accelerator controls pedal (1).

Important: The throttle should operate freely without binding between full closed and wide open throttle.

4. Check for complete throttle opening and closing positions by operating the accelerator controls pedal. Also check for poor carpet fit under the accelerator controls pedal.
5. Install the left closeout/insulator pane. Refer to Instrument Panel Insulator Panel Replacement - Left Side