For 1990-2009 cars

## Transmission Mount Replacement Trans Mount

### Removal Procedure

#### Tools Required

J 28467-360

1. Remove the engine frame. Refer to Frame Removal in Frame and Underbody.
2. Remove the mount (1) from the mount bracket.

### Installation Procedure

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

1. Install the right transmission mount (1) into the mount bracket and install the mount nuts.

Tighten
Tighten the mount nuts to 50 N·m (37 lb ft).

2. Install the engine frame. Refer to Frame Removal

## Transmission Mount Replacement Transaxle Mount

### Removal Procedure

1. Raise the vehicle. Support the vehicle. Refer to Lifting and Jacking the Vehicle in General Information.
2. Support the transmission with a jackstand.
3. Remove the bolt attaching the torque strut to the torque strut bracket.
4. Remove the bolts attaching the torque strut to the transmission.
5. Remove the torque strut.

### Installation Procedure

1. Install the torque strut into the bracket.

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

2. Install the bolts attaching the torque strut to the transmission.

Tighten
Tighten the bolts to 55 N·m (41 lb ft).

3. Install the bolt attaching the torque strut to the torque strut bracket.
4. Remove the jackstand.
5. Lower the vehicle.