For 1990-2009 cars

• | Important: Parts that are to be reused must be marked, sorted, and organized for assembly.
- Mark, sort, and organize the components for assembly.

• | Caution: Bodily injury may occur if the cleaning solvent is inhaled or exposed to the skin. Caution: Wear safety glasses in order to avoid eye damage.
- Clean the components with cleaning solvent.

• |
- Dry the components with compressed air.

• |
- Inspect the valve rocker components for the following:

- | Valve rocker arm valve pushrod socket contact surface (1)

- | The contact surface must be smooth with no scoring or excessive wear.

- | Valve rocker arm roller pivot for binding or damage (2)

- | Valve rocker arm valve stem contact surface (3)

- | The contact surface should be smooth with no scoring or excessive wear.

• |
- Inspect the valve pushrods for the following:

- | Restriction of the oil passage (1)

- | Wear or scoring of the end contact surfaces (2)

- | The end contact surfaces must be smooth with no scoring or excessive wear.

- | Shaft for bends (3)

- | Roll the valve pushrod on a flat surface to determine if the valve pushrod is bent.