For 1990-2009 cars

## Water Pump Replacement VIN K

### Removal Procedure

Caution: Unless directed otherwise, the ignition and start switch must be in the OFF or LOCK position, and all electrical loads must be OFF before servicing any electrical component. Disconnect the negative battery cable to prevent an electrical spark should a tool or equipment come in contact with an exposed electrical terminal. Failure to follow these precautions may result in personal injury and/or damage to the vehicle or its components.

1. Disconnect the negative battery cable.
2. Drain the coolant. Refer to Cooling System Draining and Filling .
3. Remove the drive belt. Refer to Drive Belt Replacement in Engine Mechincal.
4. Remove the water pump pulley bolts.
5. Remove the water pump pulley.
6. Clean the gasket mating surfaces.

### Installation Procedure

1. Using a new gasket, install the water pump on the engine.

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

2. Install the water pump bolts.

Tighten

• | Tighten the bolts (1) to 15 N·m (11 lb ft).

• | Tighten the bolts (2) to 30 N·m (22 lb ft).

3. Install the drive belt. Refer to Drive Belt Replacement in Engine Mechincal.
4. Fill the coolant. Refer to Cooling System Draining and Filling .
5. Connect the negative battery cable.
6. Check for coolant leaks.

## Water Pump Replacement VIN 1

### Removal Procedure

Caution: Unless directed otherwise, the ignition and start switch must be in the OFF or LOCK position, and all electrical loads must be OFF before servicing any electrical component. Disconnect the negative battery cable to prevent an electrical spark should a tool or equipment come in contact with an exposed electrical terminal. Failure to follow these precautions may result in personal injury and/or damage to the vehicle or its components.

1. Disconnect the negative battery cable.
2. Remove the bolts from the A/C compressor splash shield.
3. Remove the splash shield.
4. Drain the coolant. Refer to Cooling System Draining and Filling .
5. Remove the supercharger drive belt. Refer to Drive Belt Replacement in Engine Mechincal.
6. Remove the drive belt. Refer to Drive Belt Replacement in Engine Mechincal.
7. Remove the coil pack. Position the coil pack out of the way.
8. Remove the supercharger belt tensioner. Refer to Drive Belt Tensioner Replacement in Engine Mechincal.
9. Remove the engine mount. Refer to Engine Mount Replacement in Engine Mechincal.
10. Remove the power steering pump.
11. Remove the engine mount bracket.
12. Remove the idler pulley.
13. Remove the water pump pulley.
14. Remove the water pump.
15. Clean all of the gasket mating surfaces.

### Installation Procedure

1. Using a new gasket, install the water pump on the engine.

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

2. Install the water pump bolts.

Tighten

• | Tighten the bolts (1) to 15 N·m (11 lb ft).

• | Tighten the bolts (2) to 30 N·m (22 lb ft).

3. Install the water pump pulley.

Tighten
Tighten the bolts to 13 N·m (115 lb in).

4. Install the idler pulley.
5. Install the engine mount bracket.
6. Install the power steering pump.
7. Install the engine mount. Refer to Engine Mount Replacement in Engine Mechincal.
8. Install the supercharger belt tensioner. Refer to Drive Belt Tensioner Replacement in Engine Mechincal.
9. Install the coil pack.
10. Install the accessory drive belt. Refer to Drive Belt Replacement in Engine Mechincal.
11. Install the supercharger drive belt. Refer to Drive Belt Replacement in Engine Mechincal.
12. Refill the coolant. Refer to Cooling System Draining and Filling .
13. Install the A/C compressor splash shield.
14. Connect the negative battery cable.
15. Check for coolant leaks.