For 1990-2009 cars

#### Visual Inspection

1. Before the performing the load test, visually inspect the battery for obvious damage, such as a cracked or broken case.
2. Repair the cause of any damage or replace the battery. Refer to Battery Replacement .

#### Hydrometer Check

1. If the green dot is visible (A), perform the load test. Refer to Battery Load Test .
2. If the green dot is not visible (B), charge the battery. Refer to Battery Charging .
3. If the dot is clear or yellow (C), replace the battery. Refer to Battery Replacement .