For 1990-2009 cars

1. Remove the fuel injector sight shield. Refer to Fuel Injector Sight Shield Replacement in Engine Mechanical.

Important: The adjustment lock (1) is located on the TBI end of the cable.

2. Disengage the adjustment lock (1) on the cruise control cable.

When the adjustment lock is disengaged, the cable will move freely in and out of the adjuster.

3. Hold the TBI at the closed position.
4. Complete the following steps in order to eliminate slack in the cable:

4.1. | Pull the cable.

4.2. | Engage the adjustment lock.

5. Install the fuel injector sight shield. Refer to Fuel Injector Sight Shield Replacement in Engine Mechanical.