For 1990-2009 cars

Step | Action | Value(s) | Yes | No
--- | --- | --- | --- | ---
1 | Did you perform the Instrument Cluster System Check? | -- | Go to Step 2 | Go to Instrument Cluster System Check
2 |

1. Disconnect the rear compartment lid latch switch connector.
2. Turn the ignition switch to the RUN position.

Does the TRUNK AJAR indicator remain illuminated?

--

Go to Step 3

Go to Step 4

3 | Inspect for a short to ground in CKT 744 (RED/BLK). Is the wiring OK? | -- | Go to Step 6 | Go to Step 5
4 | Inspect the rear compartment lid latch switch for proper terminal contact. Is the terminal contact OK? | -- | Go to Step 8 | Go to Step 7
5 | Repair the short to ground in CKT 744 (RED/BLK). Did you complete the repair? | -- | Go to Instrument Cluster System Check | --
6 | Replace the instrument cluster. Did you complete the repair? | -- | Go to Instrument Cluster System Check | --
7 | Repair the poor terminal contact. Did you complete the repair? | -- | Go to Instrument Cluster System Check | --
8 | Replace the rear compartment lid latch switch. Did you complete the repair? | -- | Go to Instrument Cluster System Check | --