For 1990-2009 cars

## Front Seat Armrest Replacement Storage

### Removal Procedure

1. Remove the seat. Refer to Seat Replacement .
2. Remove the HVAC duct (3) at the armrest, if applicable.
3. Remove the hog rings (3) from the seat cushion flap (2) on the underside of the seat
4. Remove the following components:

• | The 4 nuts (1)

• | The armrest

### Installation Procedure

1. Install the following components:

• | The 4 nuts (1)

• | The armrest (1)

2. Install the hog rings (3) to the seat cushion flap (2) on the underside of the seat.
3. Install the HVAC duct (3) at the armrest, if applicable.
4. Install the seat. Refer to Seat Replacement .

## Front Seat Armrest Replacement Center with foam

### Removal Procedure

1. Remove the seat from the vehicle.
2. Remove the fasteners (3) that attach the armrest (1).
3. Remove the armrest (1).

### Installation Procedure

1. Install the armrest (1).
2. Install the fasteners (3) to the armrest (1).
3. Install the seat into the vehicle.