For 1990-2009 cars

### Removal Procedure

1. Open the rear compartment lid.
2. Remove the push-in fasteners (2) retaining the compass module to the rear shelf in the rear compartment.
3. Slide the module (1) from the mounting slot.
4. Disconnect the connector (3).

### Installation Procedure

1. Connect the connector (3) to the module (1).
2. Install the module into the mounting slot.
3. Install the push-in fasteners (2).

Press the push-in fasteners until firmly seated.

4. Close the rear compartment lid.