For 1990-2009 cars

Checks | Action
--- | ---
DEFINITION: Engine delivers less than expected power. Little or no increase in speed when the accelerator pedal is pushed down part way.
Preliminary Checks |

• | Refer to Powertrain On Board Diagnostic (OBD) System Check .

• | Refer to Important Preliminary Checks Before Starting in Symptoms .

• | Refer to Visual/Physical Checks in Symptoms .

• | Search for bulletins.

Fuel System |

• | Check the fuel pressure.

- | Refer to Fuel System Pressure Test (VIN K) .

- | Refer to Fuel System Pressure Test (VIN 1) .

- | Refer to Engine Oil Level Sensor and/or Switch Diagnosis .

• | Check the fuel injectors.

- | Refer to Fuel Injector Solenoid Coil Test - Engine Coolant Temperature Between 10-35 Degrees C (50-95 Degrees F) .

- | Refer to Fuel Injector Solenoid Coil Test - Engine Coolant Temperature Outside 10-35 Degrees C (50-95 Degrees F) .

• | Check for contaminated fuel. Refer to Alcohol/Contaminants-in-Fuel Diagnosis .

• | Check items which can cause an engine to run rich (long term fuel trim is significantly in the negative range). Refer to Diagnostic Aids for DTC P0172 Fuel Trim System Rich .

• | Check items that can cause an engine to run lean (long term fuel trim is significantly in the positive range). Refer to Diagnostic Aids for DTC P0171 Fuel Trim System Lean .

Sensor/System |

• | Monitor the KS system for excessive spark retard activity using a scan tool.

• | Check the EGR valve for a stuck open pintle. Refer to Exhaust Gas Recirculation Valve Replacement .

• | Check for a restricted intake duct or a dirty air cleaner element. Refer to Air Cleaner Element Replacement .

• | (VIN 1 only) -- Check for proper supercharger boost control operation. Refer to Boost Control System Diagnosis .

Ignition System |

• | Check for proper ignition voltage output using the following steps:

- | Clip the spark tester J 26792 to engine ground.

- | Connect one end of a spark plug wire to the spark tester; leave the other end of the spark plug wire to the coil being tested.

- | Connect one end of another spark plug wire to the other coil tower; connect the other end of the spark plug wire to ground.

- | Crank the engine while observing the spark tester; a spark should be observed.

- | Repeat the above steps for each coil.

• | If spark is not present at the coil(s), check for the following conditions:

| Important: If carbon tracking is detected on any component, replace that component and its mate.

- | Inspect the coil(s) for cracks, carbon tracking/arcing, or a secondary resistance value outside the specified range.

Coil Secondary Resistance
5000 - 8000 ohms (5K - 8K ohms)

- | Inspect the spark plug wires for signs of arcing/cross firing, cracks, carbon tracking, plug boot damage, pinched, incorrect routing, or a resistance value greater than the specified value.

VIN 1 Spark Plug Wires Resistance
3280 - 4921 ohms per meter (1000 ohms - 1500 ohms per foot)

VIN K Spark Plug Wires Resistance
3280 - 4921 ohms per meter (1000 ohms - 1500 ohms per foot)

| Important: Spraying the secondary ignition wires with a light mist of water may help locate an intermittent problem. Ignition components will arc to ground when a secondary component is malfunctioning.

- | Check for a malfunctioning ignition control module.

- | Check the ignition system wiring for a loose ignition module feed, ground connection, or damaged system wiring.

• | Remove the spark plugs.

• | Inspect the spark plugs for the following conditions:

- | Check the spark plug(s) for fouling. Refer to Spark Plug Visual Diagnosis .

- | Check the spark plug for cracks.

- | Refer to Spark Plug Visual Diagnosis .

| Important: If carbon tracking is detected on any component, replace that component and its mate.

- | Check the spark plugs for signs of carbon tracking on the porcelain or arching at the plug wire contact. Refer to Spark Plug Visual Diagnosis .

- | Check the spark plugs for incorrect gap. Refer to Spark Plug Visual Diagnosis .

- | Check the spark plugs for burned or damaged electrodes. Refer to Spark Plug Visual Diagnosis .

- | Check the spark plugs for incorrect heat range. Refer to Maintenance Items .

• | If spark plugs are gas or oil fouled, the cause of the fouling must be determined before replacing the spark plugs. Refer to Spark Plug Visual Diagnosis .

Engine Mechanical |

• | Check for excessive oil in combustion chamber-Leaking valve seals. Refer to Oil Consumption Diagnosis

• | Inspect for low cylinder compression. Refer to Cylinder Leakage Test

• | For incorrect basic engine parts, inspect the following. Refer to Engine Overhaul .

- | Camshaft

- | Cylinder heads

- | Pistons, etc.

Additional Checks |

• | Check the exhaust system for a possible restriction.

- | Inspect the exhaust system for damaged or collapsed pipes.

- | Inspect the muffler for heat distress or possible internal failure.

- | Check for a plugged three-way catalytic converter. Refer to Restricted Exhaust System Check and/or Restricted Exhaust .

• | Check for proper TCC operation. Refer to Functional Test .