For 1990-2009 cars

1. Lubricate the pivot pin (2) with sythetic grease. Install the pivot pin (2).
2. Pull the pivot and pulse switch assembly (1) through the column.
3. Pull the pivot and pulse switch assembly through the column.
4. Slide the pivot and pulse switch connector into the bulk head connector.
5. Reconnect the pivot and pulse switch assembly to the fused jumper assembly.
6. Install the housing cover assembly. Refer to Steering Column Jacket - Assemble - Off Vehicle .