For 1990-2009 cars

## Range Selector Lever Cable Replacement New Cable Installation

1. Set the parking brake.
2. Block the wheels.
3. Place the transaxle in the Neutral position.
4. Place the shift control in the Neutral position.
5. Connect each cable section to the following before connecting the two cable sections:

• | To the automatic transaxle range selector lever and shift cable bracket.

• | To the column or the console shift control and retainer or wiring harness clip.

6. Insert the metal end fitting of the shift control cable into the transaxle cable end.
7. Use the molded end fittings to push the metal end fitting of the shift control cable and the transaxle cable end together until the metal post snaps into place.
8. Depress the adjuster clip once. This mobilizes the adjuster housing toward the transaxle end fitting.
9. Line up the end fittings so they slide together until you feel the parts cam together and lock.
10. Depress the adjuster clip completely. This locks the cable into its adjusted service position.
11. Pull the conduit in the opposite direction to assure full system adjustment of the shift cable.

Important: The horseshoe clip with the tab is flush when fully engaged.

12. Ensure the conduit is fully engaged.
13. The horseshoe clip with the tab is not flush when not fully engaged.
14. Install the shift cable retainer and the wiring harness clip or the wiring harness strap.

## Range Selector Lever Cable Replacement AT PNP Switch

### Removal Procedure

1. Remove the throttle body air inlet duct. Refer to Engine Controls.
2. Remove the automatic transaxle range selector cable from the wiring harness clip or strap.
3. Remove the automatic transaxle range selector cable from the automatic transaxle range selector lever.
4. Remove the automatic transaxle range selector cable from the automatic transaxle range selector cable bracket.
5. Remove the automatic transaxle range selector cable from the console shift control or the column shift control. Refer to Range Selector Lever Cable Replacement
6. Pull the automatic transaxle range selector cable through the dash from the engine compartment side.

### Installation Procedure

Caution: The automatic transaxle range selector cable is made out of two cable sections. After initial connection never separate the two metal couplings from one another. Integrity of the connection of the two metal couplings will be lost if separation of the two metal couplings occurs. When servicing the transaxle remove the cable at the automatic transaxle range selector lever and at the automatic transaxle range selector cable bracket. If either section of the cable needs to be replaced, replace both of the cable sections. Loss of connection integrity of the two metal couplings can cause loss of transaxle shift control which could result in personal injury.

1. Insert the automatic transaxle range selector cable through the dash from the engine compartment side.
2. Install the automatic transaxle range selector cable to the automatic transaxle range selector cable bracket.
3. Install the automatic transaxle range selector cable to the automatic transaxle range selector lever.
4. Install the automatic transaxle range selector cable to the wiring harness clip or strap.
5. Install the automatic transaxle range selector cable to the console shift control . Refer to Range Selector Lever Cable Replacement .
6. Adjust the automatic transaxle range selector cable. Refer to Range Selector Lever Cable Replacement .
7. Install theAir ncleaner intake duct. Refer to Air Cleaner Intake Duct Replacement Engine Controls.

## Range Selector Lever Cable Replacement AT Console Switch

### Removal Procedure

1. Remove the automatic transaxle range selector cable from wiring harness clip(s) or retainer(s) in the engine compartment.
2. Remove the console. Refer to Instrument panel, Gages and Console.
3. Pull the carpet back to expose the automatic transaxle range selector cable. Refer to Seats and Carpet.
4. Remove the automatic transaxle range selector cable from retaining clip(s) or retainer(s) in the passenger compartment.
5. Disengage the automatic transaxle range selector cable retainer to the console shift control.
6. Remove the automatic transaxle range selector cable retainer from the console shift control.
7. Remove the automatic transaxle range selector cable from the console shift control.
8. Remove the automatic transaxle range selector cable through the hole in the cowl.
9. Remove the automatic transaxle range selector cable from the PNP switch. Refer to Range Selector Lever Cable Replacement .

### Installation Procedure

Caution: The automatic transaxle range selector cable is made out of two cable sections. After initial connection never separate the two metal couplings from one another. Integrity of the connection of the two metal couplings will be lost if separation of the two metal couplings occurs. When servicing the transaxle remove the cable at the automatic transaxle range selector lever and at the automatic transaxle range selector cable bracket. If either section of the cable needs to be replaced, replace both of the cable sections. Loss of connection integrity of the two metal couplings can cause loss of transaxle shift control which could result in personal injury.

1. Properly route and position the automatic transaxle range selector cable.
2. Install the automatic transaxle range selector cable through the hole in the cowl.
3. Install the automatic transaxle range selector cable to the PNP switch. Refer to Range Selector Lever Cable Replacement .
4. Install the automatic transaxle range selector cable through the console shift control bracket.
5. Install the automatic transaxle range selector cable to the console shift control.
6. Engage the automatic transaxle range selector cable retainer to the console shift control.
7. Install the automatic transaxle range selector cable to retaining clip(s) or retainer(s) in the passenger compartment.
8. Install the carpet into position. Refer to Seats and Carpet.
9. Install the console. Refer to Instrument panel, Gages and Console.
10. Install the automatic transaxle range selector cable to wiring harness clip(s) or retainer(s) in the engine compartment.
11. Adjust the automatic transaxle range selector cable. Refer to Range Selector Lever Cable Replacement and/or Park/Neutral Position Switch Adjustment .