For 1990-2009 cars

### Removal Procedure

1. Remove the headlamp. Refer to Headlamp Replacement .
2. Remove the screw (1) that retains the cornering lamp (2) to the fender.
3. Turn the socket counterclockwise in order to remove the socket from the cornering lamp (2).
4. Remove the cornering lamp (2).

### Installation Procedure

1. Install the socket to the cornering lamp (2).
2. Install the cornering lamp (2) assembly.
3. Install the screw (1) in order to retain the cornering lamp (2) to the fender.
4. Install the headlamp. Refer to Headlamp Replacement .