For 1990-2009 cars

## Instrument Panel Inflatable Restraint Module Replacement Buick

### Removal Procedure

Caution: When you are carrying an undeployed inflator module:

• | Do not carry the inflator module by the wires or connector on the inflator module

• | Make sure the bag opening points away from you

When you are storing an undeployed inflator module, make sure the bag opening points away from the surface on which the inflator module rests. When you are storing a steering column, do not rest the column with the bag opening facing down and the column vertical. Provide free space for the air bag to expand in case of an accidental deployment. Otherwise, personal injury may result.

1. Disable the SIR system. Refer to Disabling the SIR System .
2. Remove the IP trim plate. Refer to Instrument Panel, Gauges, and Console.
3. Remove the inflatable restraint IP module mounting fasteners (2,3).
4. Remove the inflatable restraint IP module (4) from the IP (1).
5. Fully deploy the module before disposal. If the module was replaced under warranty, fully deploy and dispose of the module after the required retention period. Refer to Inflator Module Handling, Shipping, and Scrapping .

### Installation Procedure

1. Route the pigtail (5) down through the IP (1).
2. Slide the inflatable restraint IP module (4) into the IP opening (1).
3. Install all of the inflatable restraint IP module mounting fasteners.

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

Tighten

• | Tighten the nuts to 10 N·m (84 lb in).

• | Tighten the bolts to 11 N·m (94 lb in).

4. Install the IP Trim Plate. Refer to Instrument Panel, Gauges, and Console.
5. Enable the SIR system. Refer to Enabling the SIR System .

## Instrument Panel Inflatable Restraint Module Replacement Oldsmobile

### Removal Procedure

Caution: When you are carrying an undeployed inflator module:

• | Do not carry the inflator module by the wires or connector on the inflator module

• | Make sure the bag opening points away from you

When you are storing an undeployed inflator module, make sure the bag opening points away from the surface on which the inflator module rests. When you are storing a steering column, do not rest the column with the bag opening facing down and the column vertical. Provide free space for the air bag to expand in case of an accidental deployment. Otherwise, personal injury may result.

1. Disable the SIR system. Refer to Disabling the SIR System .
2. Remove the IP upper trim pad. Refer to Instrument Panel, Gauges, and Console.
3. Remove the inflatable restraint IP module mounting fasteners (3).
4. Remove the inflatable restraint IP module (1) from the IP (2).
5. Fully deploy the module before disposal. If the module was replaced under warranty, fully deploy and dispose of the module after the required retention period. Refer to Inflator Module Handling, Shipping, and Scrapping .

### Installation Procedure

1. Route the pigtail (4) down through the IP (2).
2. Slide the inflatable restraint IP module (1) into the IP opening.
3. Install all of the inflatable restraint IP module mounting fasteners.

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

Tighten
Tighten fasteners to 16 N·m (12 lb ft).

4. Install the upper IP. Refer to Instrument Panel, Gauges, and Console.
5. Enable the SIR system. Refer to Enabling the SIR System .

## Instrument Panel Inflatable Restraint Module Replacement Pontiac

### Removal Procedure

Caution: When you are carrying an undeployed inflator module:

• | Do not carry the inflator module by the wires or connector on the inflator module

• | Make sure the bag opening points away from you

When you are storing an undeployed inflator module, make sure the bag opening points away from the surface on which the inflator module rests. When you are storing a steering column, do not rest the column with the bag opening facing down and the column vertical. Provide free space for the air bag to expand in case of an accidental deployment. Otherwise, personal injury may result.

1. Disable the SIR system. Refer to Disabling the SIR System .
2. Remove the IP assembly. Refer to Instrument Panel, Gauges, and Console.
3. Remove the inflatable restraint IP module mounting bolts (7,8).
4. Remove the inflatable restraint IP module mounting nuts (6,5,4,3,2,1).
5. Remove the inflatable restraint IP module (4) from the IP (1).
6. Fully deploy the module before disposal. If the module was replaced under warranty, fully deploy and dispose of the module after the required retention period. Refer to Inflator Module Handling, Shipping, and Scrapping .

### Installation Procedure

1. Slide the inflatable restraint IP module (4) into the IP opening.
2. Install all of the inflatable restraint IP module mounting fasteners.

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

Tighten

• | Tighten the nuts, in the proper order (1 to 6), to 10 N·m (84 lb in).

• | Tighten the bolts, in the proper order (7 and 8) to 2 N·m (17 lb in).

3. Install the IP Assembly. Refer to Instrument Panel, Gauges, and Console in Body and Accessories.
4. Enable the SIR system. Refer to Enabling the SIR System .