For 1990-2009 cars

# COOLING FAN RELAY CONTACTS STICKING (FAN REMAINS ON)

#### SUBJECT COOLING FAN RELAY CONTACTS STICKING (REPLACE WITH NEW COOLING FAN RELAY)

#### MODELS/YEARS 1988-90 EIGHTY-EIGHT AND NINETY-EIGHT MODELS

#### CONDITION:

Cooling fan relay contacts stick causing the cooling fan to run continuously.

#### CORRECTION:

A new cooling fan relay has been developed for the subject vehicles. The new relay uses silver-tin oxide contacts to reduce contact sticking.

To correct this condition, replace the cooling fan relay using part number 25553347. This new relay will require replacing the original fan relay bracket using part number 25558149.

Parts are currently available from GMSPO.

#### WARRANTY INFORMATION:

Labor Operation No.: T5204 Labor Time: 0.2 hour Trouble Code: 92

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.