For 1990-2009 cars

Step | Action | Value(s) | Yes | No
--- | --- | --- | --- | ---
1 | Did you perform the Cigar Lighter/Auxiliary Outlets System Check? | -- | Go to Step 2 | Go to Cigar Lighter/Auxiliary Outlets System Check
2 | Measure the voltage from the cigar lighter terminal A and ground. Is the voltage within the specified range? | 10-15 V | Go to Step 7 | Go to Step 3
3 | Check the CIGAR LTR fuse. Is the fuse OK? | -- | Go to Step 4 | Go to Step 5
4 | Check circuit 440 (ORN) from the IP fuse block to the cigar lighter for an open. Is there an open in the circuit? | -- | Go to Step 6 | Go to Step 7
5 | Repair the short to ground in circuit 440 (ORN). Is the repair complete? | -- | Go to Cigar Lighter/Auxiliary Outlets System Check | --
6 | Repair the open or poor connection in circuit 440 (ORN). Is the repair complete? | -- | Go to Cigar Lighter/Auxiliary Outlets System Check | --
7 | Measure the voltage from the cigar lighter terminal A and terminal B. Is the voltage within the specified range? | 10-15 V | Go to Step 8 | Go to Step 9
8 | Replace the cigar lighter. Is the repair complete? | -- | Go to Cigar Lighter/Auxiliary Outlets System Check | --
9 | Repair the open or poor connection in circuit 1250 (BLK). Is the repair complete? | -- | Go to Cigar Lighter/Auxiliary Outlets System Check | --