For 1990-2009 cars

1. Loosen the lock nuts on the tie rod.

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

Notice: Care must be taken that the boots are not twisted when rotating the inner tie rods, or damage to the boots may result.

2. Rotate the inner tie rod to adjust the toe. Refer to Wheel Alignment Specifications .

Tighten
Tighten the lock nuts to 64 N·m (47 lb ft).

3. Adjust the boots as needed in order to prevent damage.