For 1990-2009 cars

# INFO. ON THE OPERATION OF TURN SIGNAL REMINDER CHIME

#### SUBJECT: INFORMATION ON THE OPERATION OF TURN SIGNAL REMINDER CHIME

#### MODELS: 1996 OLDSMOBILE LSS WITH GAUGES CLUSTER (RPO UH8) 1996 OLDSMOBILE NINETY EIGHT WITH DIGITAL CLUSTER (RPO U2A)

THE TURN SIGNAL REMINDER CHIME TURNS ON WHEN THE VEHICLE HAS TRAVELED 3/4 MILE WITH A TURN SIGNAL ON. FOR THE ABOVE LISTED VEHICLES, THIS CHIME SOUNDS ONLY FOUR TIMES INSTEAD OF CONTINUOUSLY. THIS CHANGE IN THE OPERATION OF THE TURN SIGNAL REMINDER CHIME IS THE RESULT OF A SOFTWARE CHANGE.

FIGURES: 00 ATTACHMENTS: 00

GENERAL MOTORS BULLETINS ARE INTENDED FOR USE BY PROFESSIONAL TECHNICIANS, NOT A "DO-IT-YOURSELFER". THEY ARE WRITTEN TO INFORM THOSE TECHNICIANS OF CONDITIONS THAT MAY OCCUR ON SOME VEHICLES, OR TO PROVIDE INFORMATION THAT COULD ASSIST IN THE PROPER SERVICE OF A VEHICLE. PROPERLY TRAINED TECHNICIANS HAVE THE EQUIPMENT, TOOLS, SAFETY INSTRUCTIONS AND KNOW-HOW TO DO A JOB PROPERLY AND SAFELY. IF A CONDITION IS DESCRIBED, DO NOT ASSUME THAT THE BULLETIN APPLIES TO YOUR VEHICLE, OR THAT YOUR VEHICLE WILL HAVE THAT CONDITION. SEE A GENERAL MOTORS DEALER SERVICING YOUR BRAND OF GENERAL MOTORS VEHICLE FOR INFORMATION ON WHETHER YOUR VEHICLE MAY BENEFIT FROM THE INFORMATION.

COPYRIGHT 1996 GENERAL MOTORS CORPORATION. ALL RIGHTS RESERVED.