For 1990-2009 cars

# SMU-SEC.9J SIR CAUTION REVISED SYS. TESTER CAUTION

DIVS INVL 3 7

THIS BULLETIN IS BEING REVISED TO INCLUDE THE 1991 H CAR.

THE CAUTION ON PAGE 5 OF SECTION 9J IN THE 1990 EIGHTY-EIGHT/ NINETY-EIGHT SERVICE MANUAL AS WELL AS THE 1991 EIGHTY-EIGHT SERVIC MANUAL HAS BEEN REVISED TO CORRECT THE CORRESPONDENCE OF THE MODEL YEAR TO THE APPROPRIATE VEHICLE MODEL. THE CAUTION REFERS TO MODEL YEARS 1988-1991. WHEN USING J 36884-A REFER TO THE FOLLOWING CAUTION FOR PROPER APPLICATIONS.

#### CAUTION:

THE SUPPLEMENTAL INFLATABLE RESTRAINT SYSTEM TESTER J 36884A IS A SPECIAL PURPOSE TESTER DESIGNED TO BE USED WITH THE 1988, 1989, AND 1990 OLDSMOBILE NINETY-EIGHT AND THE 1988, 1989, 1990, AND 1991 OLDSMOBILE EIGHTY-EIGHT ONLY. THE TESTER IS USED TO DETERMINE WHETHER OR NOT A SPECIFIC PART OR THE ENTIRE SYSTEM IS FUNCTIONING PROPERLY. USE OF OTHER TEST EQUIPMENT COULD RESULT IN PERSONAL INJURY.

PLEASE UPDATE YOUR SERVICE MANUALS ACCORDINGLY.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.

-COPYRIGHT 1991 GENERAL MOTORS CORPORATION. ALL RIGHTS RESERVED.