For 1990-2009 cars

### Removal Procedure

#### Tools Required

J 25034-C Pulley Remover

1. Remove the pump drive belts. Refer to Drive Belt Replacement in Engine Mechanical.
2. Remove the pump from the engine. Refer to Power Steering Pump Replacement .
3. Use the J 25034-C in order to remove the pulley from the pump.

### Installation Procedure

#### Tools Required

J 25033-C Pulley Installer

1. Use the J 25033-C in order to install the pulley onto the pump.
2. Axial tolerance of the pulley on the pump shaft is -0.25 mm to 0.25 mm (-0.010 in to 0.010 in).
3. Install the pump to the engine. Refer to Power Steering Pump Replacement .
4. Install the pump drive belt. Refer to Drive Belt Replacement in Engine Mechanical.
5. Bleed the power steering system.
6. Inspect the system for leaks.