For 1990-2009 cars

## Front Bumper Fascia Air Deflector Replacement Buick

### Removal Procedure

1. Raise and support the vehicle. Refer to Lifting and Jacking the Vehicle in General Information.
2. Remove the screws that retain the lower air deflector (4) to the front bumper fascia (1).
3. Remove the lower air deflector (4).

### Installation Procedure

1. Install the lower air deflector (4).
2. Install the screws in order to retain the lower air deflector (4) to the front bumper fascia (1).
3. Lower the vehicle.

## Front Bumper Fascia Air Deflector Replacement Pontiac

### Removal Procedure

1. Raise and support the vehicle. Refer to Lifting and Jacking the Vehicle in General Information.
2. Remove the screws (5) that retain the lower air deflector (4).
3. Remove the lower air deflector (4).

### Installation Procedure

1. Install the lower air deflector (4).
2. Install the screws (5) in order to retain the lower air deflector (4).
3. Lower the vehicle.

## Front Bumper Fascia Air Deflector Replacement Oldsmobile

### Removal Procedure

1. Raise and support the vehicle. Refer to Lifting and Jacking the Vehicle in General Information.
2. Remove the bolts (4) that attach the lower air deflector (3) to the fascia supports (2,6).
3. Remove the bolts (4) that attach the lower air deflector to the front bumper fascia (1).

### Installation Procedure

1. Install the bolts (4) in order to connect the lower air deflector (3) to the front bumper fascia (1).
2. Install the bolts (4) in order to attach the lower air deflector to the fascia supports (2,6).
3. Lower the vehicle.