For 1990-2009 cars

# BACK GLASS REPLACEMENT 3H-69 STYLES

BACK GLASS REPLACEMENT

#### VEHICLES AFFECTED 1986 Oldsmobile 3H69 Styles ----------------- Willow Run Production Only

On Oldsmobile 3H69 styles, from VIN lG3HN6931GW328328 through lG3HY69LOGW332023 a back glass for vinyl top equipped vehicles was also used on non-vinyl top vehicles.

If replacement of the back glass is necessary on a vehicle within the above VIN number sequence, the following vinyl top style glass must be used:

Part No. 20321454 Heated Part No. 20321453 Nonheated

The removal and installation procedure is the same as outlined in the service manual.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.