For 1990-2009 cars

### Removal Procedure

Important: There is no service interval for in-line fuel filter replacement. Only replace the in-line fuel filter if it is restricted.

1. Relieve the fuel system pressure. Refer to the Fuel Pressure Relief .
2. Raise the vehicle.
3. Remove the quick-connect fitting at the fuel feed line (2). Refer to Servicing Quick Connect Fittings .
4. Remove the threaded connection (5) at in-line fuel filter (1).
5. Inspect the fuel lines, O-rings for cuts, swelling, cracks, and distortion. Replace the lines as required.
6. Inspect the fuel return line (3).
7. Inspect the fuel vent pipe (4).
8. Drain any remaining fuel into an approved gasoline container.

### Installation Procedure

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

1. Remove the protective caps from the new in-line fuel filter.
2. Install the new plastic connector retainers on the in-line fuel filter inlet and outlet.

Install the new plastic connector retainers in the same position as on the old in-line fuel filter.

3. Install the quick-connect fitting (2) at the inlet of the in-line fuel filter. Refer to Servicing Quick Connect Fittings .
4. Install the threaded connection (5) at the in-line fuel filter (1).
5. Lower the vehicle.
6. Tighten the fuel tank filler pipe cap.
7. Install the negative battery cable.

7.1. | Turn the ignition switch ON for 2 seconds.

7.2. | Turn the ignition switch OFF for 10 seconds.

7.3. | Turn the ignition switch ON

7.4. | Check for fuel leaks.