For 1990-2009 cars

### Removal Procedure

1. Remove the air distributor assembly. Refer to Air Distributor Duct Replacement
2. Remove the bolts (2) that attach the air inlet (3) to the dash panel (1) and to the front of the dash.
3. Reposition the insulation as needed to remove the air inlet assembly (3).

### Installation Procedure

1. Position the air inlet (3) in the vehicle.
2. Reposition the insulation as needed.

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

3. Install the bolts (2) to attach the air inlet (3) to the dash panel (1) and to the front of the dash.

Refer to the illustration for the proper tightening sequence.

Tighten
Tighten the bolts to 5 N·m (44 lb in).

4. Install the air distributor assembly. Refer to Air Distributor Duct Replacement