For 1990-2009 cars

## SECURITY Indicator Always On or Flashing Engine Starts

Step | Action | Yes | No
--- | --- | --- | ---
1 | Did you perform the Vehicle Theft Deterrent (VTD) System Check? | Go to Step 2 | Go to Vehicle Theft Deterrent (VTD) System Check
2 | Perform a lock cylinder and key test usingJ 35628-A Interrogator. Did the test pass? | Go to Step 3 | Go to Step 8
3 |

1. Turn the ignition switch to OFF.
2. Disconnect the Theft Deterrent Module Connector.
3. Turn the ignition switch to RUN.

Does the SECURITY indicator turn OFF?

Go to Theft Deterrent Module Replacement

Go to Step 4

4 | Is the vehicle equipped with content theft deterrent (UA6)? | Go to Step 5 | Go to Step 6
5 | Disconnect the remote function actuator (RFA) module connector. Does the SECURITY indicator turn OFF? | Go to Step 7 | Go to Step 6
6 | Repair short to ground in CKT 264. Refer to Wiring Repairs in Wiring Systems. Is the repair complete? | Go to Vehicle Theft Deterrent (VTD) System Check | --
7 | Replace the RFA module. Refer to Remote Control Door Lock Receiver Replacement . Is the replacement complete? | Go to Vehicle Theft Deterrent (VTD) System Check | --
8 | Repair short to ground or open in circuits 1073 or 1074. Refer to Wiring Repairs in Wiring Systems. Did you find and correct the condition? | System OK | Go to Ignition Lock Cylinder Replacement - On Vehicle

## SECURITY Indicator Always On or Flashing Engine Does Not Crank

Step | Action | Value(s) | Yes | No
--- | --- | --- | --- | ---
1 | Did you perform the Vehicle Theft Deterrent (VTD) System Check? | -- | Go to Step 2 | Go to Vehicle Theft Deterrent (VTD) System Check
2 | Test the key in the J 35628-A J Interrogator. Is the key code valid? | -- | Go to Step 4 | Go to Step 3
3 |

1. Clean the key.
2. Retest the key in the J 35628-A Interrogator.

Is the key code valid?

--

Go to Content Theft Deterrent (CTD) System Check

Go to Step 17

4 |

1. Connect both of the J 35628-90 Adaptor Harness 48-way connectors to C202.
2. Connect both J 35628-90 2-way connector to the J 35628-A Interrogator.
3. Test the lock cylinder with the following procedure:

3.1. | With the proper key, rotate the ignition lock cylinder through all positions.

3.2. | While rotating, observe the key code display for any variance in key code number.

3.3. | Repeat the procedure multiple times to verify any intermittent concerns.

Does the display change to another key code value or E at any position?

--

Go to Step 6

Go to Step 5

5 |

1. Turn the ignition switch to OFF.
2. Disconnect the J 35628-90 Adaptor Harness and the J 35628-A Interrogator.
3. Measure the resistance from connector C202 (ignition lock side) terminal E13 to ground.

Is the resistance within the specified range?

OL

Go to Step 19

Go to Step 6

6 | Replace the ignition lock cylinder and keys. Refer to Ignition Lock Cylinder Replacement - On Vehicle Is the repair complete? | -- | Go to Content Theft Deterrent (CTD) System Check | --
7 |

1. Reconnect connector C202.
2. Measure the resistance across the key pellet. Record the value.
3. Put the key into the ignition lock cylinder.
4. Disconnect the theft deterrent module connector.
5. Measure the resistance from the theft deterrent module harness connector terminal B7 to terminal B8.

Does the resistance measure within the specified range of the key pellet resistance?

0-10 ohms

Go to Step 10

Go to Step 8

8 | Inspect connector C202 terminal E12 and terminal E13 for proper connections. Refer to Intermittents and Poor Connections Diagnosis in Wiring Systems. Are the connections OK? | -- | Go to Step 9 | Go to Step 20
9 | Repair either of the following circuits for an open or high resistance between connector C202 and the theft deterrent module connector:

• | CKT 1073 (WHT/BLK)

• | CKT 1074 (PPL/WHT). Refer to Wiring Repairs in Wiring Systems.

Is the repair complete?

--

Go to Content Theft Deterrent (CTD) System Check

--

10 |

1. Place the key in the ignition lock cylinder in the OFF position.
2. Measure the resistance from the theft deterrent module harness connector terminal B8 to ground.

Is the resistance less than or equal to the specified value?

OL

Go to Step 11

Go to Step 21

11 | Repair a short to ground in CKT 1073 (WHT/BLK) between connector C202 at the base of the steering column and the theft deterrent module connector. Refer to Wiring Repairs in Wiring Systems. Is the repair complete? | -- | Go to Content Theft Deterrent (CTD) System Check | --
12 | Inspect the ground to the theft deterrent module harness connector for proper connections. Refer to Intermittents and Poor Connections Diagnosis in Wiring Systems. Are the terminal contacts OK? | -- | Go to Step 13 | Go to Step 23
13 |

1. Reconnect the theft deterrent module connector.
2. Try to start the engine.

Does the engine start?

--

Go to Step 15

Go to Step 14

14 |

1. Turn the ignition switch to ON.
2. Observe the security indicator.

Does the indicator turn off after 3 minutes?

--

Go to Step 16

Go to Step 18

15 | Inspect connector C202 for proper connection. Refer to Intermittents and Poor Connections Diagnosis in Wiring Systems. Is the terminal contact OK? | -- | Go to Step 24 | Go to Step 20
16 | Try to start the engine with a spare key. Does the engine start? | -- | Go to Step 17 | Go to Step 18
17 |

1. Replace the suspect key.
2. Match the key code with the spare key.

Is the replacement complete?

--

Go to Content Theft Deterrent (CTD) System Check

--

18 | Replace the theft deterrent module. Refer to Theft Deterrent Module Replacement Is the replacement complete? | -- | Go to Content Theft Deterrent (CTD) System Check | --
19 |

1. Turn the ignition OFF.
2. Measure the resistance from connector C202 (ignition lock side) terminal E12 to ground.

Is the resistance within the specified range?

OL

Go to Step 7

Go to Step 6

20 | Repair poor terminal contact. Refer to Wiring Repairs in Wiring Systems. Is the repair complete? | -- | Go to Content Theft Deterrent (CTD) System Check | --
21 |

1. Turn the ignition OFF.
2. Measure the resistance from the theft deterrent module harness connector terminal B7 to ground.

Is the resistance less than or equal to the specified range?

OL

Go to Step 12

Go to Step 22

22 | Repair a short to ground in CKT 1074 (PPL/WHT) between connector C202 at the base of the steering column and the theft deterrent module. Refer to Wiring Repairs in Wiring Systems. Is the repair complete? | -- | Go to Content Theft Deterrent (CTD) System Check |
23 | Repair the ground to the theft deterrent module. Refer to Wiring Repairs in Wiring Systems. Is the repair complete? | -- | Go to Content Theft Deterrent (CTD) System Check |
24 | Inspect the theft deterrent module connectors for proper contact. Refer to Intermittents and Poor Connections Diagnosis in Wiring Systems. Is the terminal contact OK? | -- | Go to Content Theft Deterrent (CTD) System Check | Go to Step 20