For 1990-2009 cars

## Sun Load Temperature Sensor Replacement Buick

### Removal Procedure

1. Remove the defroster grille by prying up on the grille.
2. Remove the sun load sensor (1) from the defroster grille by twisting the sensor ¼ turn.
3. Disconnect the sun load sensor electrical connector.
4. Remove the sun load sensor (1).

### Installation Procedure

1. Connect the sun load sensor electrical connector.
2. Install the sun load sensor (1) to the defroster grille by twisting the sensor ¼ turn.
3. Install the defroster grille by snapping the grille into place.

## Sun Load Temperature Sensor Replacement Oldsmobile

### Removal Procedure

1. Remove the defroster grille (2) by prying up on the grille.
2. Remove the sun load sensor (1) from the defroster grille (2) by twisting the sensor ¼ turn.
3. Disconnect the sun load sensor electrical connector.
4. Remove the sun load sensor (1).

### Installation Procedure

1. Connect the sun load sensor electrical connector.
2. Install the sun load sensor (1) to the defroster grille (2) by twisting the sensor ¼ turn.
3. Install the defroster grille (2) by snapping the grille into place.

## Sun Load Temperature Sensor Replacement Pontiac

### Removal Procedure

1. Remove the defroster grille by prying up on the grille.
2. Remove the sun load sensor (1) from the defroster grille by twisting the sensor ¼ turn.
3. Disconnect the sun load sensor electrical connector.
4. Remove the sun load sensor (1).

### Installation Procedure

1. Connect the sun load sensor electrical connector.
2. Install the sun load sensor (1) to the defroster grille by twisting the sensor ¼ turn.
3. Install the defroster grille by snapping the grille into place.