For 1990-2009 cars

#### Tools Required

J 34115 Left Side Axle Seal Installer

Notice: Install the seal onto the tool before installing into the case to prevent damage to the seal.

Important: When you remove a drive axle from the transmission for any reason, inspect the axle sealing surface (tripot shank) for corrosion. If corrosion is evident, clean the surface with a 320 grit cloth or equivalent. Clean off any remaining debris with automatic transmission fluid. Wipe the surface dry and reinstall the drive axle free of any build up.

Use J 34115 in order to install the left side axle oil seal assembly (409).