For 1990-2009 cars

## Intake Manifold Installation Upper

1. Install the upper intake manifold. Make sure to install the two hidden bolts in the lower intake manifold.
2. Install the upper intake manifold bolts.

Tighten
Tighten the bolts in sequence to 10 N·m (89 lb in).

Refer to

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

in General Information.
3. Install the throttle body.
4. Install the cable bracket to the intake manifold.
5. Install the fuel rail.
6. Install the ignition wires to the fuel rail.
7. Install the spark plug wires on the right side of the engine.

## Intake Manifold Installation Lower

1. Install the lower intake manifold gasket.
2. Install the lower intake manifold.
3. Apply Threadlocker 272 GM P/N 12345493 to the bolt threads.
4. Install the lower intake manifold bolts.

Tighten
Tighten the bolts in sequence to 15 N·m (11 lb ft).

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

5. Make sure to install the two hidden bolts.
6. Install the EGR outlet pipe to the intake manifold.
7. Install the EGR outlet pipe bolt.

Tighten
Tighten the EGR outlet pipe bolt to 29 N·m (21 lb ft).