For 1990-2009 cars

## Front Seat Lumbar Support Replacement AM1,AM2

### Removal Procedure

1. Remove the seat with the aid from an assistant. Refer to one of the following procedures:

Seat Replacement

Seat Replacement

2. Place the seat upside down on a clean, protected surface.
3. Remove the adjuster bolts (2) and the adjuster assembly (4).
4. Remove the lumbar knob (1). Refer to Lumbar Support Knob Replacement .
5. Remove the lumbar adjuster.

### Installation Procedure

1. Install the lumbar adjuster.
2. Install the lumbar knob (1). Refer to Lumbar Support Knob Replacement .
3. Install the seat adjuster assembly (4) and bolts (2).

Caution: Unless directed otherwise, the ignition and start switch must be in the OFF or LOCK position, and all electrical loads must be OFF before servicing any electrical component. Disconnect the negative battery cable to prevent an electrical spark should a tool or equipment come in contact with an exposed electrical terminal. Failure to follow these precautions may result in personal injury and/or damage to the vehicle or its components.

4. Install the adjuster assembly bolts.

Tighten
Tighten the adjuster assembly bolts to 24 N·m (17 lb ft).

5. With the aid from an assistant, install the seat. Refer to Seat Replacement .