For 1990-2009 cars

### Removal Procedure

1. Remove the weather-strip (1) from the flange.
2. Remove all traces of adhesive from around the perimeter of the opening.

### Installation Procedure

1. Install the weather-strip (1) to the flange.
2. Inspect the weather-stripping (1) in order to verify that the clinch is completely seated to the flange around the entire opening.
3. Using a hose with no nozzle attached, test the weather-strip (1) in order to verify that no leaks are present. If leaks are present, remove the weather-strip.
4. Brush Goodwrench Weather-strip Adhesive P/N 123145097, 3M 08011, or the equivalent around the perimeter of the flange.