For 1990-2009 cars

### Removal Procedure

1. Remove the rear compartment lid trim. Refer to Rear Compartment Lid Inner Panel Trim Replacement .
2. Remove the rear compartment lid latch. Refer to Rear Compartment Lid Latch Replacement .
3. Disconnect the electrical connectors.
4. Remove the bolt that retains the actuator to the latch (2).
5. Remove the actuator.

### Installation Procedure

1. Install the actuator to the latch (2).
2. Install the bolt in order to retain the actuator.
3. Connect the electrical connectors.
4. Install the rear compartment lid latch to the rear compartment lid. Refer to Rear Compartment Lid Latch Replacement
5. Install the rear compartment lid trim. Refer to Rear Compartment Lid Inner Panel Trim Replacement