For 1990-2009 cars

The MAF sensor on this engine is attached to the throttle body assembly.

### Removal Procedure

1. Disconnect the MAF sensor electrical connector.
2. Remove the screws holding MAF sensor to throttle body.
3. Remove the MAF sensor from the throttle body.

### Installation Procedure

1. Carefully position the MAF sensor to the throttle body.
2. Install 3 screws holding the MAF sensor to the throttle body.
3. Connect the electrical connector.