For 1990-2009 cars

1. Remove the key from the ignition switch.
2. Connect the inflatable restraint IP module yellow 2-way connector (2). The connector is located above the right sound insulator.
3. Attach the inflatable restraint IP module yellow 2-way connector (2) to the IP sound insulator (1) (Pontiac).
4. Attach the inflatable restraint IP module yellow 2-way connector to the IP (2) (Buick).
5. Attach the inflatable restraint IP module yellow 2-way connector (3) to the IP sound insulator (1) (Oldsmobile).
6. Install the connector position assurance (CPA) (2) to the inflatable restraint IP module yellow 2-way connector (1). The connector is located above the right sound insulator.
7. Install the right sound insulator. Refer to Instrument Panel Insulator Panel Replacement - Right Side in Instrument Panel, Gauges, and Console.
8. Connect the inflatable restraint steering wheel yellow 2-way connector (1,3). The connector is located near the base of the steering column.
9. Install the connector position assurance (CPA) (3) to the inflatable restraint steering wheel yellow 2-way connector (1). The connector is located near the base of the steering column.
10. Install the left sound insulator. Refer to Instrument Panel Insulator Panel Replacement - Left Side in Instrument Panel, Gauges, and Console.
11. Install the AIR BAG fuse in the IP fuse block.

Important: Ensure that you remain a safe distance from both of the air bags.

12. Turn the ignition switch to the RUN position. The following actions should occur:

12.1. | The AIR BAG warning lamp will flash 7 times.

12.2. | The AIR BAG warning lamp will then turn OFF.

13. Perform the SIR diagnostic system check. Refer to SIR Diagnostic System Check .