For 1990-2009 cars

### Removal Procedure

1. Remove the air distributor assembly. Refer to Air Distributor Duct Replacement .
2. Unclip the defrost-A/C actuator (3) from the air inlet.
3. Disengage the defrost-A/C actuator (3) from the valve.

### Installation Procedure

1. Engage the defrost-A/C actuator (3) to the valve.
2. Clip the defrost-A/C actuator (3) to the air inlet.
3. Install the air distributor assembly. Refer to Air Distributor Duct Replacement .