For 1990-2009 cars
Engine Controls Components
VIN K Fuel Conrol
OBD II Symbol Description Notice
Handling ESD Sensitive Parts Notice
Handling ESD Sensitive Parts Notice

### Circuit Description

The PASS-Key II ® module produces the Theft Deterrent Fuel Enable signal when ignition is ON and the proper key resistor pellet is sensed by the PASS-Key II ® module. The PCM monitors the Fuel Enable signal during crank. If the proper signal is present on the Theft Deterrent Fuel Enable circuit, the PCM enables fuel delivery to allow the engine to start. If the PCM detects that the fuel enable signal is not present or is incorrect while an attempt is made to start the engine, DTC P1629 will be set. The engine will not start as long as this condition is present. If the problem also affects inputs to the PASS-Key II ® module, the starter motor may be disabled. If this condition is present, refer to Theft Deterrent Systems for further diagnosis.

### Conditions for Setting the DTC

• | DTC P1626 is not present.

• | An attempt is made to start the engine.

• | The PCM detects an incorrect signal on the theft deterrent fuel enable circuit.

• | The above conditions are present for longer than 2 seconds.

### Action Taken When the DTC Sets

• | The PCM will not illuminate the malfunction indicator lamp (MIL).

• | The PCM will store conditions which were present when the DTC set as Failure Records data only. This information will not be stored as Freeze Frame data.

### Conditions for Clearing the MIL/DTC

• | A History DTC will clear after 40 consecutive warm-up cycles have occurred without a malfunction.

• | The DTC can be cleared by using the scan tool Clear Info function.

### Diagnostic Aids

An intermittent may be caused by a poor connection, rubbed through wire insulation or a wire broken inside the insulation. Check for:

• | Poor connection. Inspect the PCM and Vehicle Theft Deterrent module harness and connectors for improper mating, broken locks, improperly formed or damaged terminals, and poor terminal to wire connection.

• | Damaged harness. Inspect the wiring harness for damage. If the harness appears to be OK, disconnect the vehicle theft deterrent module, turn the ignition ON and observe a digital multimeter connected to the theft deterrent fuel enable circuit at the vehicle theft deterrent module harness connector while moving connectors and wiring harnesses related to the vehicle theft deterrent system. A change in voltage will indicate the location of the malfunction.

Reviewing the Fail Records vehicle mileage since the diagnostic test last failed may help determine how often the condition that caused the DTC to be set occurs. This may assist in diagnosing the condition.

### Test Description

Number(s) below refer to the step number(s) on the Diagnostic Table.

1. This vehicle is equipped with a PCM which utilizes an Electrically Erasable Programmable Read Only Memory (EEPROM). When the PCM is being replaced, the new PCM must be programmed.

#### DTC P1629 - Theft Deterrent System Fuel Enable Circuit Incorrect Signal Detected During Crank

Step | Action | Value(s) | Yes | No
--- | --- | --- | --- | ---
1 | Was the Powertrain On-Board Diagnostic (OBD) System Check performed? | -- | Go to Step 2 | Go to the Powertrain On Board Diagnostic (OBD) System Check
2 | Important:: Before continuing diagnosis, ensure that the vehicle battery is fully charged. Attempt to start the engine. Does the engine crank? | -- | Go to Step 3 | Go to Vehicle Theft Deterrent System in Electrical Diagnosis.
3 |

1. Turn OFF the ignition switch.
2. Disconnect the vehicle theft deterrent module.
3. Turn ON the ignition switch.
4. Using a J 39200 Digital Multimeter, measure voltage between the vehicle theft deterrent fuel enable circuit and the ground circuit at the vehicle theft deterrent module harness connector.

Does voltage measure near the specified value?

5 V

Go to Step 4

Go to Step 6

4 |

1. Turn OFF the ignition switch.
2. Reconnect the vehicle theft deterrent module.
3. Turn ON the ignition switch.
4. Backprobe the vehicle theft deterrent module connector to measure frequency between the vehicle theft deterrent fuel enable circuit and ground.

Is the frequency between the specified values?

40-60 Hz

Go to Step 5

Go to Step 8

5 |

1. Turn ON the ignition switch.
2. Clear DTC P1629.
3. Attempt to start the vehicle.

Does the vehicle start and continue running?

--

Refer to Diagnostic Aids

Go to Step 7

6 |

1. Check the vehicle theft deterrent fuel enable circuit for an open, short to ground, or short to voltage.
2. If a problem is found, repair as necessary. Refer to Repair Procedures in Electrical Diagnosis.

Was a problem found?

--

Go to Step 11

Go to Step 7

7 |

1. Check the theft deterrent fuel enable circuit for a poor connection at the PCM.
2. If a problem is found, replace terminal. Refer to Repair Procedures in Electrical Diagnosis.

Was a problem found?

--

Go to Step 11

Go to Step 9

8 |

1. Check for poor connections at the theft deterrent module.
2. If a problem is found, replace terminal(s). Refer to Repair Procedures in Electrical Diagnosis.

Was a problem found?

--

Go to Step 11

Go to Step 10

9 | Replace the PCM. Important:: The replacement PCM must be programmed. Refer to Powertrain Control Module Replacement/Programming . Is action complete? | -- | Go to Step 11 | --
10 | Replace the vehicle theft deterrent module. Refer to On-Vehicle Service in Theft Deterrent Systems Is action complete? | -- | Go to Step 11 | --
11 |

1. Clear DTCs.
2. Observe VTD Fuel Disable on the scan tool while cranking the engine.

Does VTD Fuel Disable display Active?

--

Go to Step 2

System OK