For 1990-2009 cars

# BATTERY DRAIN, BATTERY IS LOW OR DEAD (REPL. LH FRONT

#### SUBJECT: BATTERY DRAIN, BATTERY IS LOW OR DEAD (REPLACE LH FRONT OUTSIDE MIRROR SWITCH)

#### MODELS: 1995-96 OLDSMOBILE NINETY EIGHT REGENCY ELITE WITH A43 1997-98 OLDSMOBILE REGENCY

#### CONDITION:

SOME OWNERS MAY COMMENT THAT THE BATTERY IS LOW OR DEAD. ALSO, A CLICKING NOISE MAY BE HEARD COMING FROM THE MEMORY SEAT/MIRROR MODULE LOCATED UNDER THE SEAT.

#### CAUSE:

THE LH FRONT MIRROR SWITCH CAN REACH AN INDETERMINENT STATE WHICH MAY CAUSE THE MEMORY SEAT/MIRROR MODULE TO WAKE-UP AND THEN GO TO SLEEP REPEATEDLY. A CLICKING NOISE MAY BE HEARD COMING FROM THE MODULE. THE REPEATED WAKING-UP OF THE MEMORY SEAT/MIRROR MODULE CAUSES A BATTERY DRAIN.

#### CORRECTION:

REPLACE THE LH FRONT OUTSIDE MIRROR SWITCH, P/N 25681297.

#### PARTS INFORMATION:

PARTS ARE CURRENTLY AVAILABLE FROM GMSPO.

#### WARRANTY INFORMATION:

FOR VEHICLES REPAIRED UNDER WARRANTY, USE:

LABOR OPERATION LABOR OPERATION NUMBER DESCRIPTION TIME --------------- ----------- ---------------

R3318 SWITCH, ELECTRIC REMOTE USE PUBLISHED LABOR CONTROL MIRROR - REPLACE OPERATION TIME

FIGURES: 00 ATTACHMENTS: 00

GENERAL MOTORS BULLETINS ARE INTENDED FOR USE BY PROFESSIONAL TECHNICIANS, NOT A "DO-IT-YOURSELFER". THEY ARE WRITTEN TO INFORM THOSE TECHNICIANS OF CONDITIONS THAT MAY OCCUR ON SOME VEHICLES, OR TO PROVIDE INFORMATION THAT COULD ASSIST IN THE PROPER SERVICE OF A VEHICLE. PROPERLY TRAINED TECHNICIANS HAVE THE EQUIPMENT, TOOLS, SAFETY INSTRUCTIONS AND KNOW-HOW TO DO A JOB PROPERLY AND SAFELY. IF A CONDITION IS DESCRIBED, DO NOT ASSUME THAT THE BULLETIN APPLIES TO YOUR VEHICLE, OR THAT YOUR VEHICLE WILL HAVE THAT CONDITION. SEE A GENERAL MOTORS DEALER SERVICING YOUR BRAND OF GENERAL MOTORS VEHICLE FOR INFORMATION ON WHETHER YOUR VEHICLE MAY BENEFIT FROM THE INFORMATION.

COPYRIGHT 1998 GENERAL MOTORS CORPORATION. ALL RIGHTS RESERVED.