For 1990-2009 cars

## Drive Belt Tensioner Replacement VIN 1

### Removal Procedure

1. Remove the supercharger belt.
2. Remove the ignition module.
3. Remove the tensioner bolts.
4. Remove the tensioner.

### Installation Procedure

1. Install the tensioner.
2. Install the tensioner bolts.

Tighten
Tighten the bolts to 50 N·m (37 lb ft).

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

3. Install the ignition module.
4. Install the supercharger belt.

## Drive Belt Tensioner Replacement VIN K

### Removal Procedure

1. Disconnect the negative battery cable. Refer to

   Caution: Unless directed otherwise, the ignition and start switch must be in the OFF or LOCK position, and all electrical loads must be OFF before servicing any electrical component. Disconnect the negative battery cable to prevent an electrical spark should a tool or equipment come in contact with an exposed electrical terminal. Failure to follow these precautions may result in personal injury and/or damage to the vehicle or its components.

   in General Information.
2. Raise the vehicle.
3. Remove the front lower splash shield.
4. Drain the coolant. Refer to SECTION 6B.
5. Close the radiator drain cock.
6. Install the front splash shield.
7. Lower the vehicle.
8. Remove the accessory drive belt.
9. Remove the generator. Refer to SECTION 6D3.
10. Remove the heater hoses.
11. Remove the drive belt tensioner bolts.
12. Remove the drive belt tensioner.

### Installation Procedure

1. Install the drive belt tensioner. Refer to Drive Belt Tensioner Installation
2. Install the drive belt tensioner bolts. Refer to Drive Belt Tensioner Installation

Tighten
Tighten the drive belt bolts to 50 N·m (37 lb ft).

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

3. Install the heater hoses.
4. Install the generator. Refer to SECTION 6D3.
5. Install the accessory drive belt. Refer to Accessory Drive Belts Replacement
6. Refill the coolant. Refer to SECTION 6B.
7. Connect the negative battery cable.