For 1990-2009 cars

### Removal Procedure

1. Disconnect the electrical connector from the EGR valve.
2. Remove the 2 EGR valve retaining nuts (4).
3. Remove the EGR valve (1).
4. Remove the gasket (2) from the EGR valve adapter (3).

### Installation Procedure

1. Install a new gasket (2) on the EGR adapter (3).

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

2. Install the EGR valve (1) and two nuts (4).

Tighten
Tighten the nuts to 30 N·m (22 lb ft).

3. Connect the EGR valve electrical connector.