For 1990-2009 cars

# MAINTENANCE SCHEDULE BOOKLETS NEW AND UPDATED INFORMATION

#### MODELS/YEARS: ALL 1987 MODELS

All 1987 Oldsmobile vehicles have a maintenance schedule booklet installed in the car at the time of production. Each booklet has two schedules of service intervals (Schedule I and II below). The schedule the owner should follow depends on how the car is driven.

There has been some new and updated maintenance and lubrication information for the 1987 model year. Please read Section 0B in the 1987 New Product Service Manual for a full explanation of all maintenance service required.

Some of the new items are:

o The 1987 Maintenance Schedules now list the recommended intervals for tire and wheel rotation.

o No EGR system service is required on 3.0L and 3.8L engines.

o 4 section type new power antenna assembly does not require lubrication.

Schedule I is to be followed if the car is mainly driven under one or more of the following conditions:

o When most trips are less than 4 miles (6 kilometers).

o When most trips are less than 10 miles (16 kilometers) and outside temperatures remain below freezing.

o Idling and/or low-speed operation in stop-and-go traffic.

o Towing a trailer.

o Operating in dusty areas.

Schedule I should also be followed if the car is used for delivery service, police, taxi or other commercial applications.

Schedule II is to be followed ONLY if none of the driving conditions specified in Schedule I apply.

If a maintenance booklet is lost, additional booklets are available through your Zone Office. The part number is as follows:

Maintenance Schedule Part Number ------------------- ----------- GM Passenger Car 14102712

----------------------------------------------------------------------------- Schedule I

Follow Schedule I if your car is mainly driven under one or more of the following conditions:

When most trips are less than 4 miles (6 kilometers).

When most trips are less than 10 miles (16 kilometers) and outside temperatures remain below freezing.

Item To Be Services When to Perform No. Miles (kolometers) or Months, --- -------------- Whichever Occurs First ----------------------- 1 Engine oil & oil filter change * Every 3,000 mi.(5,000 km) or 3 mos.

2 Chassis lubrication Every other oil change.

3 Carburetor choke & hose inspection At 6,000 mi (10,000 km) and (if equipped)* then at each 30,000 mi. (50,000 km) interval

4 Carburetor or throttle body At 6,000 mi.(10,000 km) only mounting bolt torque*

5 Engine idle speed adjustment (some models) *

6 Tire & wheel rotation At 6,000 mi.(10,000 km) and then every 15,000 mi. (25,000 km)

7 Vacuum or A.I.R. pump drive Every 30,00 mi.(50,000 km) belt inspection * or 24 mos.

8 Cooling system service *

9 Wheel bearing repack (rear wheel drive cars only See explanation on page 7. 10 Transmission/transaxle service

11 Vacuum advance system inspection Every 30,000 mi.(50,000 km) 12 Spark plug and wire service *

13 PCV valve inspection *

14 EGR system service * Every 30,000 mi.(50,000 km) or 36 mos. 15 Air cleaner & PCV filter replacement*

16 Engine timing check (some models) *

17 Fuel tank, cap & lines inspection * Every 30,000 mi. (50,000 km)

18 Thermostatically controlled air cleaner inspection (some models)*

* An emission control service

** In California, these are the minimum Emission Control Maintenance Services an owner must perform according to the California Air Resources Board. General Motors, however, urges that all Emission Control Maintenance Services shown be performed. to maintain your other new car warranties, all services shown in this booklet should be performed.

- Idling and/or low-speed operation in stop-and-go traffic.***

- Towing a trailer.

- Operating in dusty areas.

The service shown in this schedule up to 48,000 miles (80 000 km) are to be performed after 48,000 miles at the same intervals.

MILES (000) 3 6 9 12 15 18 21 24 27 30 33 36 39 42 45 48 KILOMETERS (000) 5 10 15 20 25 30 35 40 45 50 55 60 65 70 75 80

1 - - - - - - - - - - - - - - - - 2 - - - - - - - - 3 - -** 4 -** 5 -** 6 - - - 7 -** 8 - 9 10 11 - 12 -** 13 - 14 - 15 -** 16 - 17 - 18 -

*** Note: Schedule I should also be followed if the car is used for delivery service, police, taxi or other commercial applications. ----------------------------------------------------------------------------- Schedule II

Follow Schedule II only if none of the driving conditions specified on Schedule I apply.

Item To Be Serviced When to Perform No. Miles (kilometers) or Months, -- --------------- Whichever Occurs First ---------------------- 1 Engine oil change (Turbocharged, Every 7,5000 mi.(12 500 km) see ***)* or 12 mos. Oil filter change * *** At first and then every other oil change or 12 mos.

2 Chassis lubricaiton Every 7,500 mi.(12 500 km) or 12 mos.

3 Carburetor choke & hose inspection At 7,500 mi. (12 500 km) and (if equipped) * then at each 3,000 mi. (50 000 km) interval

4 Carburetor or throttle body At 7,500 mi.(12 500 km) only mounting bolt torque *

5 Engine idle speed adjustment (some models)*

6 Tire & wheel rotation At 7,500 mi. (12 500 km) and then every 15,000 mi (25 000 km)

7 Vacuum or A.I.R. Pump drive belt inspection * Every 30,000 mi. (50 000 km) or 24 mos. 8 Cooling system service *

9 Wheel bearing repack (rear-wheel Every 30,000 mi. (50 000 km) drive cars only)

10 Transmission/transaxle service See explanation on page 7.

11 Vacuum advance system inspection (some models) * Every 30,000 mi. (50 000 km) 12 Spark Plug and Wire Service* 13 PCV Valve Inspection *

14 EGR system service * Every 30,000 mi.(50 000 km) 15 Air cleaner & PCV filter replacement * or 36 mos.

16 Engine timing check (some models)* 17 Fuel tank, cap & lines inspection * Every 30,000 mi.(50 000 km) 18 Thermostatically controlled air cleaner inspection (some models).*

* An Emission Control Service

** In California, these are the minimum Emission Control Maintenance Services an owner must perform according to the California Air Resources Board. General Motors, however, urges that all Emission Control Maintenance Services shown be performed. to maintain your other new car warranties, all services shown in this booklet should be performed.

The services shown in this schedule up to 45,000 miles (75 000 km) are to be performed after 45,000 miles at the same intervals.

MILES (000) 7.5 15 22.5 30 37.5 45 KILOMETERS (000) 12.5 25 37.5 50 62.5 75

1 - - - - - - - - - 2 - - - - - - 3 - -** 4 -** 5 -** 6 - - - 7 -** 8 - 9 - 10 11 - 12 -** 13 - 14 - 15 -** 16 - 17 - 18 -

*** Turbocharged engines.

- VIN engine code M - change oil every 3,000 miles (5 000 km) or 3 months, whichever comes first. Change engine oil filter at first oil chang, then every other oil change.

- VIN engine code 7 - change oil and filter every 7,500 miles (12 500 km) or 12 months, whichever comes first.

#### NOTE: To determine engine code and displacement, see the Specifications Section of your Owner's Manual.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.