For 1990-2009 cars

### Removal Procedure

1. Remove the door lock switch bezel. Refer to Front Side Door Trim Panel Insert Replacement .
2. Release the power seat switch retainers.

Use a small, flat-bladed tool.

3. Disconnect the electrical connectors.
4. Remove the power seat switch.

### Installation Procedure

1. Align the power seat switch with the door lock bezel.
2. Install the power seat switch to the bezel.

Push downward on the switch.

3. Connect the electrical connectors.
4. Install the door lock switch bezel. Refer to Front Side Door Trim Panel Insert Replacement .