For 1990-2009 cars

1. Remove the indicated control valve body bolts (374-381, 384).
2. Carefully lift the fluid pressure manual valve position switch assembly (395) off of the control valve body (300). Handle the switch assembly carefully, it is very delicate.
3. Remove the control valve body assembly (300).
4. Remove the two retainers (368) from the valve body assembly.
5. Remove the spacer plate assembly (370) with the two screen/seal assemblies (382) and the gaskets (369, 371) from the valve body (300).

• | Remove the six ball check valves (372, 373) from the valve body (300).

• | Remove the case cover pin (410).

6. Remove the four ball check valves (372) from the case cover (400).