For 1990-2009 cars

### Removal Procedure

1. Ensure that the lever (4) is in the center, or the OFF position.
2. Remove the access cover (1) from the steering column housing.
3. Disconnect the cruise control wiring connector (2).

Note the position of the connector installed in the column.

4. Pull the lever (4) straight out of the turn signal switch.

### Installation Procedure

1. Be sure that the lever (4) is in the center, or the OFF position.
2. Push the lever (4) into the turn signal switch.
3. Connect the cruise control wiring connector (2).
4. Install the access cover (1) to the steering column housing.