For 1990-2009 cars

### Removal Procedure

1. Remove the right closeout/insulator panel. Refer to Instrument Panel Insulator Panel Replacement - Right Side .
2. Remove the left closeout/insulator panel. Refer to Instrument Panel Insulator Panel Replacement - Left Side .
3. Slide the LCM to the left from the retainer while holding onto the lock tab.
4. Disconnect the electrical connectors.

### Installation Procedure

1. Electrical connectors to the LCM.
2. Slide the LCM into the retainer, push to the right to engage.
3. Install the left closeout/insulator panel. Refer to Instrument Panel Insulator Panel Replacement - Left Side .
4. Install the right closeout/insulator panel. Refer to Instrument Panel Insulator Panel Replacement - Right Side .