For 1990-2009 cars

### Removal Procedure

1. Open the vanity cover.
2. Use a thin-bladed tool in order to disengage the 2 front snap legs at the lower edge of the sunshade.
3. Pull the vanity out and downward in order to access the electrical connections.

Important: Note the wire routing for installation.

4. Disconnect the wire connectors from the vanity, if equipped.
5. Remove the vanity mirror.

### Installation Procedure

1. Connect the wire connectors, if equipped.
2. Insert the top end of the vanity into the sunshade.
3. Firmly apply pressure to engage the snap legs.
4. Close the vanity mirror cover.