For 1990-2009 cars

1. Using a small screwdriver, pry the wiring harness (224) electrical connectors off of the following components:

• | Automatic transaxle fluid pressure manual valve position switch assembly (395)

• | 1-2, 3-4 Shift solenoid valve assembly (315A)

• | 2-3 Shift solenoid valve assembly (315B)

• | TCC PWM solenoid valve assembly (334)

• | Pressure control solenoid valve assembly (322)

• | Automatic transaxle input speed sensor assembly (440)

2. Gently pull the automatic transaxle fluid temperature sensor (391) from it's clip.
3. Lift the wiring harness assembly (224) off of the transaxle.