For 1990-2009 cars

### Removal Procedure

Important: The internal circuit board is replaceable. The terminals and housing are part of the wiring harness.

1. Remove the right sound insulator. Refer to Instrument Panel Insulator Panel Replacement - Right Side in Instrument Panel, Gauges and Console.
2. Unsnap the brake lamp driver module from the MALL bracket.
3. Open the brake lamp driver module endcap (1) and remove the circuit board by pulling straight out.

### Installation Procedure

1. Carefully install the circuit board into the brake lamp driver module case and close the endcap (1).
2. Snap the brake lamp driver module into the MALL bracket clip.
3. Install the right sound insulator. Refer to Instrument Panel Insulator Panel Replacement - Right Side in Instrument Panel, Gauges and Console.