For 1990-2009 cars

Step | Action | Value(s) | Yes | No
--- | --- | --- | --- | ---
1 | Did you perform the Exterior Lights System Check? | -- | Go to Step 2 | Go to Exterior Lights System Check
2 |

1. Backprobe the turn signal flasher connector with a test lamp from cavity A (PNK) to ground.
2. Turn the ignition switch to the RUN position.

Does the test lamp light?

--

Go to Step 3

Go to Step 7

3 |

1. Disconnect the turn signal flasher connector.
2. Connect a fused jumper from the turn signal flasher connector cavity A (PNK) to cavity B (PPL).
3. Place the multi-function lever in the position to indicate a left hand turn.

Do all of the left turn lamps light but not flash?

--

Go to Step 4

Go to Step 5

4 | Replace the turn signal flasher. Refer to one of the following procedures:

• | Instrument Panel Insulator Panel Replacement - Left Side

• | Instrument Panel Insulator Panel Replacement - Left Side

• | Instrument Panel Insulator Panel Replacement - Left Side

Is the repair complete?

--

Go to Exterior Lights System Check

--

5 | Inspect for an open in CKT 16 (PPL) between the turn signal flasher and the turn/hazard switch. Refer to Testing for Continuity in Wiring Systems. Is CKT 16 OK? | -- | Go to Step 6 | Go to Step 8
6 | Replace the turn/hazard switch. Refer to Hazard Warning Switch Replacement in Steering Wheel and Column - Tilt. Is the repair complete? | -- | Go to Exterior Lights System Check | --
7 | Repair the open in CKT 539 (PNK) between the IP fuse block and the turn signal flasher. Refer to Wiring Repairs in Wiring Systems. Is the repair complete? | -- | Go to Exterior Lights System Check | --
8 | Repair the open in CKT 16 (PPL) between the turn signal flasher and the turn/hazard switch. Refer to Wiring Repairs in Wiring Systems. Is the repair complete? | -- | Go to Exterior Lights System Check | --