For 1990-2009 cars

### Removal Procedure

1. Remove the bezel handle opening cover.

Use a small, flat-bladed tool.

2. Release the retainers at the top of the switch bezel.

Use a small, flat-bladed tool.

3. Pull the bezel from the door.

Disconnect the electrical connector.

4. Remove the bezel.

### Installation Procedure

1. Connect the electrical connector.
2. Align the bezel with the trim panel.
3. Align the lock rod with the lock rod knob.
4. Install the bezel to the trim panel.

Push inward the top of the bezel.

5. Install the bezel handle opening cover.