For 1990-2009 cars

### Removal Procedure

Caution: When working with any type of glass or sheet metal with exposed or rough edges, wear approved safety glasses and gloves in order to reduce the chance of personal injury.

1. Lower the glass 3 cm (1 in).
2. Remove the trim panel. Refer to Rear Side Door Trim Panel Replacement .
3. Remove the water deflector. Refer to Door Water Deflector Replacement .
4. Remove the inner sealing strip. Refer to Rear Door Window Belt Inner Sealing Strip Replacement .
5. Remove the outer belt sealing strip. Refer to Rear Door Window Belt Outer Sealing Strip Replacement .
6. Loosen the front channel assembly fastener.
7. Remove the sash fasteners (2).
8. Remove the window (1) from the outboard side.

### Installation Procedure

Caution: When working with any type of glass or sheet metal with exposed or rough edges, wear approved safety glasses and gloves in order to reduce the chance of personal injury.

1. Install the window (1) from the outboard side.
2. Install the sash fasteners (2).
3. Install the inner belt sealing strip. Refer to Rear Door Window Belt Inner Sealing Strip Replacement .
4. Install the outer belt sealing strip. Refer to Rear Door Window Belt Outer Sealing Strip Replacement .
5. Adjust the window. Refer to Rear Side Door Window Adjustment .
6. Tighten the front channel assembly upper bolt.
7. Install the water deflector. Refer to Door Water Deflector Replacement .
8. Install the trim panel. Refer to Rear Side Door Trim Panel Replacement .